**Open Geospatial Consortium**

Submission Date: 2015-12-10

Approval Date:   2016-05-25

Publication Date:   2016-12-22

External identifier of this OGC® document: <http://www.opengis.net/doc/IS/guf-xml/1.0>

Internal reference number of this OGC® document:    15-098r1

Version: 1.0

Category: OGC® Implementation Standard

Editor:   Joan Masó and Lucy Bastin

OGC Geospatial User Feedback Standard: XML Encoding Extension

**Copyright notice**

Copyright © 2016 Open Geospatial Consortium  
To obtain additional rights of use, visit <http://www.opengeospatial.org/legal/>.

**Warning**

This document is an OGC Member approved international standard. This document is available on a royalty free, non-discriminatory basis. This formatted version is INFORMATIVE. The normative format is available at:   
  
 <http://docs.opengeospatial.org/is/15-098r1/15-098r1.html>  
  
Recipients of this document are invited to submit, with their comments, notification of any relevant patent rights of which they are aware and to provide supporting documentation.

Document type:    OGC® standard

Document subtype:    Encoding

Document stage:    Approved

Document language:  English

License Agreement

Permission is hereby granted by the Open Geospatial Consortium, ("Licensor"), free of charge and subject to the terms set forth below, to any person obtaining a copy of this Intellectual Property and any associated documentation, to deal in the Intellectual Property without restriction (except as set forth below), including without limitation the rights to implement, use, copy, modify, merge, publish, distribute, and/or sublicense copies of the Intellectual Property, and to permit persons to whom the Intellectual Property is furnished to do so, provided that all copyright notices on the intellectual property are retained intact and that each person to whom the Intellectual Property is furnished agrees to the terms of this Agreement.

If you modify the Intellectual Property, all copies of the modified Intellectual Property must include, in addition to the above copyright notice, a notice that the Intellectual Property includes modifications that have not been approved or adopted by LICENSOR.

THIS LICENSE IS A COPYRIGHT LICENSE ONLY, AND DOES NOT CONVEY ANY RIGHTS UNDER ANY PATENTS THAT MAY BE IN FORCE ANYWHERE IN THE WORLD.

THE INTELLECTUAL PROPERTY IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE, AND NONINFRINGEMENT OF THIRD PARTY RIGHTS. THE COPYRIGHT HOLDER OR HOLDERS INCLUDED IN THIS NOTICE DO NOT WARRANT THAT THE FUNCTIONS CONTAINED IN THE INTELLECTUAL PROPERTY WILL MEET YOUR REQUIREMENTS OR THAT THE OPERATION OF THE INTELLECTUAL PROPERTY WILL BE UNINTERRUPTED OR ERROR FREE. ANY USE OF THE INTELLECTUAL PROPERTY SHALL BE MADE ENTIRELY AT THE USER’S OWN RISK. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR ANY CONTRIBUTOR OF INTELLECTUAL PROPERTY RIGHTS TO THE INTELLECTUAL PROPERTY BE LIABLE FOR ANY CLAIM, OR ANY DIRECT, SPECIAL, INDIRECT OR CONSEQUENTIAL DAMAGES, OR ANY DAMAGES WHATSOEVER RESULTING FROM ANY ALLEGED INFRINGEMENT OR ANY LOSS OF USE, DATA OR PROFITS, WHETHER IN AN ACTION OF CONTRACT, NEGLIGENCE OR UNDER ANY OTHER LEGAL THEORY, ARISING OUT OF OR IN CONNECTION WITH THE IMPLEMENTATION, USE, COMMERCIALIZATION OR PERFORMANCE OF THIS INTELLECTUAL PROPERTY.

This license is effective until terminated. You may terminate it at any time by destroying the Intellectual Property together with all copies in any form. The license will also terminate if you fail to comply with any term or condition of this Agreement. Except as provided in the following sentence, no such termination of this license shall require the termination of any third party end-user sublicense to the Intellectual Property which is in force as of the date of notice of such termination. In addition, should the Intellectual Property, or the operation of the Intellectual Property, infringe, or in LICENSOR’s sole opinion be likely to infringe, any patent, copyright, trademark or other right of a third party, you agree that LICENSOR, in its sole discretion, may terminate this license without any compensation or liability to you, your licensees or any other party. You agree upon termination of any kind to destroy or cause to be destroyed the Intellectual Property together with all copies in any form, whether held by you or by any third party.

Except as contained in this notice, the name of LICENSOR or of any other holder of a copyright in all or part of the Intellectual Property shall not be used in advertising or otherwise to promote the sale, use or other dealings in this Intellectual Property without prior written authorization of LICENSOR or such copyright holder. LICENSOR is and shall at all times be the sole entity that may authorize you or any third party to use certification marks, trademarks or other special designations to indicate compliance with any LICENSOR standards or specifications. This Agreement is governed by the laws of the Commonwealth of Massachusetts. The application to this Agreement of the United Nations Convention on Contracts for the International Sale of Goods is hereby expressly excluded. In the event any provision of this Agreement shall be deemed unenforceable, void or invalid, such provision shall be modified so as to make it valid and enforceable, and as so modified the entire Agreement shall remain in full force and effect. No decision, action or inaction by LICENSOR shall be construed to be a waiver of any rights or remedies available to it.

Contents

[1. Scope 6](#_Toc465090477)

[2. Conformance 7](#_Toc465090478)

[3. References 8](#_Toc465090479)

[4. Terms and Definitions 8](#_Toc465090480)

[5. Conventions 9](#_Toc465090481)

[5.1 Namespace prefix conventions 9](#_Toc465090482)

[6. Geospatial User Feedback XML encoding 9](#_Toc465090483)

[7. Geospatial User feedback model: Core 10](#_Toc465090484)

[7.1 Requirements Class Quality Common 10](#_Toc465090485)

[7.2 Requirements Class User Feedback Item 12](#_Toc465090486)

[8. Geospatial User feedback model: Extensions 16](#_Toc465090487)

[8.1 Requirements Class User Feedback Summary Extension 16](#_Toc465090488)

[8.2 Requirements Class User Feedback Collection Extension 17](#_Toc465090489)

[Annex A: Conformance Class Abstract Test Suite (Normative) 24](#_Toc465090490)

[A.1 Conformance class: Quality Common 24](#_Toc465090491)

[A.2 Conformance class: User Feedback-item 26](#_Toc465090492)

[A.3 Conformance class: Feedback-summary 26](#_Toc465090493)

[A.4 Conformance class: Feedback-collection 27](#_Toc465090494)

[Annex B: XML Schema Documents 28](#_Toc465090495)

[Annex C: Revision history 29](#_Toc465090496)

[Bibliography 30](#_Toc465090497)

Tables

Table 1 – Namespace mappings 9

Abstract

The Geospatial User Feedback XML encoding standard is based on the OGC Geospatial User Feedback conceptual model [OGC 15-097]. Geospatial User Feedback (GUF) is metadata that is predominantly produced by the consumers of geospatial data products based on their use and experience with those products. This standard complements the existing metadata conventions whereby documents recording dataset characteristics and production workflows are generated by the creator, publisher, or curator of a data product. As a part of metadata, the GUF data model internally reuses some elements of ISO 19115-1 (the updated version of the OGC Abstract Specification Topic 11) but not the general structure. This selective use of ISO metadata elements prioritizes future interoperability with developing ISO metadata models.

This standard can be used in combination with the OGC 15-097 Conceptual Model Standard. In the future, other encodings may be considered, being an alternative using the JSON-LD encoding based on parts of schema.org.

Keywords

The following are keywords to be used by search engines and document catalogues.

ogcdoc, ogc documents, user feedback, metadata, fitness-for-use, geospatial, encoding

Preface

This standard is based on work done in two European Union 7th Framework program projects called GeoViQua (FP7 FP7/2007-2013 under grant agreement n°265178) and CHARMe (FP7/2007-2013 under grant agreement n°312641). GeoViQua considers user feedback as part of the metadata that allows users to assess the quality and fitness-for-use of geospatial datasets. GeoViQua developed its quality model based on ISO 19115-1:2014 and drafts of ISO19157:2013. The GeoViQua model is divided into the Producer Quality Model and the User Feedback Model. Both models are encoded in XML based on the ISO 19139 rules. The GeoViQua User Feedback Model[[1]](#footnote-1) formed the initial basis of the model defined in this standard. CHARMe also focused on developing means for users to annotate datasets. The approach used in that project was based on W3C annotations and developed annotation conventions in RDF. Parts of the CHARMe conceptual model have been incorporated in the OGC GUF standards.

Attention is drawn to the possibility that some of the elements of this document may be the subject of patent rights. The Open Geospatial Consortium shall not be held responsible for identifying any or all such patent rights.

*Recipients of this document are requested to submit, with their comments, notification of any relevant patent claims or other intellectual property rights of which they may be aware that might be infringed by any implementation of the standard set forth in this document, and to provide supporting documentation.*

Submitting organizations

The following organizations submitted this Document to the Open Geospatial Consortium Inc.

UAB-CREAF

Aston University

Fraunhofer Institute

52 North

Submitters

All questions regarding this submission should be directed to the editor or the submitters:

|  |  |
| --- | --- |
| Name | Company |
| Joan Masó | UAB-CREAF |
| Lucy Bastin | Aston University |
| Simon Thum | Fraunhofer Institute |
| Daniel Nust | 52 North |

# Scope

This OGC® standard defines an XML encoding for encoding user feedback about geospatial datasets or metadata records describing datasets. This standard reuses and extends the ISO 19115-1:2014 model and follows the ISO 19139 encoding rules. The XML encoding is based on the Geospatial User Feedback Conceptual Model Standard [OGC 15-097].

This OGC® standard is applicable to metadata catalogue servers and clients that want to exchange geospatial user feedback information.

This OGC® standard is defined to allow implementation of catalogue clients that are able to complement the discovery of geospatial datasets. Catalogue clients present query results, commonly based on summaries of detailed metadata records created and maintained by the producers. With this standard, the metadata responses can also provide user feedback summaries and detailed user feedback reports. Clients using this standard can provide a user interface to support provision of additional comments or inquiries about datasets or to complement the producer metadata by presenting additional user feedback information about the data.

Geospatial User Feedback as used in this standard encompasses: user comments, questions and answers, user reports of dataset problems and proposed solutions to those problems, ratings, usage reports, citations of related datasets or publications describing usage, quality reports, relevant additional provenance information, and significant events related to the use or interpretation of a dataset.

This standard does not define any query language to request or send user feedback to/from metadata catalogues.

# Conformance

This standard defines 4 conformance classes.

Requirements for some standardization targets types are considered:

* Requirement Quality Common: [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/req/quality-common] has a single conformance class, Quality Common: [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/quality-common]. This conformance class targets clients and services implementing quality or user feedback models.
* Requirement Feedback-item: [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/req/feedback-item] has a single pertaining conformance class, Feedback-item [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/ feedback-item]. This conformance class targets clients and services implementing user feedback models.
* Requirement Feedback-summary: [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/req/feedback-summary] has a single conformance class, Feedback-summary:, [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/ feedback-summary]. This conformance class targets clients and services implementing user feedback models.
* Requirement Feedback-collection: [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/req/feedback-collection] has a single pertaining conformance class, Feedback-collection, [http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/ feedback-collection]. This conformance class targets clients and services implementing user feedback models.

Conformance with this standard shall be checked using all the relevant tests specified in Annex A (normative) of this document. The framework, concepts, and methodology for testing, and the criteria to be achieved to claim conformance are specified in the OGC Compliance Testing Policies and Procedures and the OGC Compliance Testing web site[[2]](#footnote-2).

All requirements-classes and conformance-classes described in this document are owned by the standard(s) identified.

# References

The following normative documents contain provisions that, through reference in this text, constitute provisions of this document. For dated references, subsequent amendments to, or revisions of, any of these publications do not apply. For undated references, the latest edition of the normative document referred to applies.

ISO / TC 211: ISO 19115-1:2014 Geographic information -- Metadata -- Part 1: Fundamentals (2014)

ISO / TC 211: ISO 19157:2013 Geographic information -- Data quality (2013)

ISO / TC 211: ISO 19139:2007 Geographic information -- Metadata -- XML schema implementation (2007)

ISO / TC 211: ISO 19115-3: Geographic information -- Metadata -- Part 3: XML schemas (2016)

OGC: OGC 15-097 Geospatial User Feedback Standard. Conceptual Model (2016)

The following candidate Standard is still under development in ISO / TC 211 and is referenced herein.

ISO / TC 211: ISO 19157-2 Geographic information -- Data quality-- Part 2: XML schemas (under development)

# Terms and Definitions

This document uses the terms defined in Sub-clause 5.3 of [OGC 06-121r8], which is based on the ISO/IEC Directives, Part 2, Rules for the structure and drafting of International Standards. In particular, the word “shall” (not “must”) is the verb form used to indicate a requirement to be strictly followed to conform to this standard.

This document uses the Terms and Definition provided by the OGC 15-097 Geospatial UserFeedback Conceptual Model standard. No additional terms and definitions apply.

# Conventions

## Namespace prefix conventions

The following namespaces are used in this document. The prefix abbreviations used constitute conventions used here, but are **not** normative. The namespaces to which the prefixes refer to are normative.

Table 1 – Namespace mappings

|  |  |  |
| --- | --- | --- |
| Prefix | Namespace URI | Description |
| xsd | <http://www.w3.org/2001/XMLSchema> | XML Schema namespace |
| gco | http://standards.iso.org/iso/19115/-3/gco/1.0 | ISO 19115 Common classes |
| mcc | http://standards.iso.org/iso/19115/-3/mcc/1.0 | ISO 19115-1 Common classes |
| mri | http://standards.iso.org/iso/19115/-3/mri/1.0 | ISO 19115-1 Identification |
| mrl | http://standards.iso.org/iso/19115/-3/mrl/1.0 | ISO 19115-1 Lineage |
| gex | http://standards.iso.org/iso/19115/-3/gex/1.0 | ISO 19115-1 Extent |
| cit | http://standards.iso.org/iso/19115/-3/cit/1.0" | ISO 19115-1 Citation |
| mdq | http://standards.iso.org/iso/19157/-2/mdq/1.0 | ISO 19157 Quality |
| lan | http://standards.iso.org/iso/19115/-3/lan/1.0 | ISO 19115-3 Language |
| qcm | http://www.opengis.net/guf/1.0/common | Quality common |
| guf | http://www.opengis.net/guf/1.0/core | User feedback core |
| ufc | http://www.opengis.net/guf/1.0/collection | User feedback collection |
| ufs | http://www.opengis.net/guf/1.0/summary | User feedback summary |
|  |  |  |

# Geospatial User Feedback XML encoding

The encoding rules for creating a XML encoding from a UML model documented in ISO 19139 were used to elaborate the XML schemas described here. These encoding rules are coded in the ShapeChange application. ShapeChange was used to automatically transform the UML model from the OGC 15-097 Geospatial User Feedback Conceptual Model into the XML schemas that are complementing this standard. Since the conversion is automatic, this document will not provide tables describing the semantics of each element and the reader should refer to the conceptual model for details.

This encoding is intended for applications where the use of producer’s metadata encoded in 19115-1:2014 is common. In this way we pave the way for extending the current ISO19115-1:2014 metadata editors and catalogues to support this model. This encoding also aims for an easy integration of the producer metadata and the user feedback in client applications.

# Geospatial User feedback model: Core

This section describes two requirements classes that are fundamental for encoding Geospatial User Feedback items in XML: the Quality Common and the User Feedback Item.

## Requirements Class Quality Common

This requirements class defines the XML encoding for data model classes that are common to, and useful for, both quality metadata generated by producers and user feedback metadata. For this reason they are kept in a separate conformance class. In essence, this conformance class represents the foundations for building a user feedback model. This requirements class inherits all the necessary elements from the ISO19115-1:2014 and the ISO19157:2013 metadata models (such as CI\_Citation, CI\_Date etc) and adds two extra classes for citing publications (QCM\_Publications) and for reporting discovery issues (QCM\_DiscoveredIssues).

1. /req/quality-common/mime-type:  
   An XML encoding of a geospatial user feedback shall adopt the XML MIME type of application/xml
2. /req/quality-common/file-extension:  
   An XML encoding of a geospatial user feedback shall use the file extension ‘.xml’
3. /req/quality-common/xmlrules:  
   An XML encoding of a geospatial user feedback shall comply with the encoding rules specified in ISO-19139.  
   Dependencies: ISO 19139
4. /req/quality-common/iso-schema:  
   An XML encoding of a geospatial user feedback shall validate using the schemas ISO19115-3 and ISO19157-2 provided at: http://standards.iso.org/iso/19115/-3 and http://standards.iso.org/iso/19157/-2 respectively  
   Dependencies: ISO 19115-3 and ISO 19157-2
5. /req/quality-common/qcm-schema:  
   An XML encoding of a geospatial user feedback using QCM\_Publication or QCM\_DiscoveredIssue shall validate using the quality common schema qcm.xsd  
   Dependencies: http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/quality-common

The qcm.xsd schema has been derived automatically from the OGC 15-097 UML model. No tables describing the naming of the elements and subelements are reproduced here as they are specified in the conceptual model.

The following code shows a xml encoding example for QCM\_Publication.

<QCM\_Publication

xmlns:cit="http://standards.iso.org/iso/19115/-3/cit/1.0"

xmlns:gco="http://standards.iso.org/iso/19115/-3/gco/1.0"

xmlns="http://www.opengis.net/guf/1.0/common"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xsi:schemaLocation="http://www.opengis.net/guf/1.0/common ../qcm.xsd">

<cit:title>

<gco:CharacterString>Exploiting synergies of global land cover products for carbon cycle modeling</gco:CharacterString>

</cit:title>

<cit:date>

<cit:CI\_Date>

<cit:date>

<gco:DateTime>2006-01-01T00:00:00Z</gco:DateTime>

</cit:date>

<cit:dateType>

<cit:CI\_DateTypeCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_DateTypeCode" codeListValue="creation"/>

</cit:dateType>

</cit:CI\_Date>

</cit:date>

<cit:series>

<cit:CI\_Series>

<cit:name>

<gco:CharacterString>Remote Sensing of Environment</gco:CharacterString>

</cit:name>

</cit:CI\_Series>

</cit:series>

<cit:otherCitationDetails>

<gco:CharacterString>101 (2006) 534–553</gco:CharacterString>

</cit:otherCitationDetails>

<motivation><QCM\_CitationMotivationCode codeListValue="descrive" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#QCM\_PublicationCategoryCode"></QCM\_CitationMotivationCode></motivation>

<category><QCM\_PublicationCategoryCode codeListValue="journalArticle" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#QCM\_PublicationCategoryCode"></QCM\_PublicationCategoryCode></category>

</QCM\_Publication>

The following code shows a xml encoding example for QCM\_DiscoveredIssue.

<QCM\_DiscoveredIssue

xmlns:gco="http://standards.iso.org/iso/19115/-3/gco/1.0"

xmlns="http://www.opengis.net/guf/1.0/common"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xsi:schemaLocation="http://www.opengis.net/guf/1.0/common ../qcm.xsd">

<knownProblem>

<gco:CharacterString>These maps cannot be used for land cover change detection since the error in the original map is higher than the change detected (e.g. GLC-2000 versus GlobCover). Due to the large disagreements between these land cover products, we recommend that the user community does not, by default, use the latest product with the highest resolution, but carefully examines the sensitivity of these products within a speciﬁc application..</gco:CharacterString>

</knownProblem>

<workAround>

<gco:CharacterString> In the situation where the maps are used for national and regional applications, we would recommend examining the disagreement of the products in the areas of interest and also to compare them with high resolution ground data or aerial photography. One way to do this would be to use geo-wiki.org (Fritz et al 2009), a global land cover validation tool, which can be used to visualize the global land cover products and the disagreement directly on top of Google Earth. By exploring the discrepancies at the level of an individual country in combination with local knowledge, the user can gain insight into which product is better in a speciﬁc region and which product is better suited for a particular application. Crowd-sourced data in the form of geo-tagged photos and information collected through Web 2.0 applications like geo-wiki and smart phones could also be harnessed as a rich source of training and calibration data for global land cover algorithms. </gco:CharacterString>

</workAround>

</QCM\_DiscoveredIssue>

## Requirements Class User Feedback Item

This requirements class defines the data model classes that are involved in the definition of an individual user feedback item. The GUF model makes an effort to remain as simple as possible but comprehensive enough to allow for simple user interfaces that can cover different levels of expertise on geospatial data usage. The following are examples of what the GUF model allows: commenting, asking questions, providing answers (the GUF\_UserComment class), rating data (GUF\_Rating), citing publications (QCM\_Publication), providing a quality measure (additionalQuality), documenting additional lineage information (additional LineageSteps), or emphasizing a significant event that conditions the interpretation of a dataset (GUF\_SignificantEvent).

Each one of the previous examples is considered an “item” of feedback. Geospatial User Every item is set into a context by a combination of target, citations and scope. Feedback can be provided both about data or metadata.

1. /req/feedback-item/guf-schema:  
   An XML encoding of a geospatial user feedback item shall use GUF\_FeedbackItem and shall validate using the geospatial user feedback item schema guf.xsd  
   Dependencies: /req/quality-common   
   http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-item

The guf.xsd schema has been derived automatically from the OGC 15-097 UML model. No tables describing the naming of the elements and subelements are reproduced here as they are specified in the conceptual model.

The following code shows a xml encoding example for GUF\_FeedbackItem.

<GUF\_FeedbackItem

xmlns:mcc="http://standards.iso.org/iso/19115/-3/mcc/1.0"

xmlns:mdq="http://standards.iso.org/iso/19157/-2/mdq/1.0"

xmlns:mri="http://standards.iso.org/iso/19115/-3/mri/1.0"

xmlns:cit="http://standards.iso.org/iso/19115/-3/cit/1.0"

xmlns:gco="http://standards.iso.org/iso/19115/-3/gco/1.0"

xmlns:qcm="http://www.opengis.net/guf/1.0/common"

xmlns="http://www.opengis.net/guf/1.0/core"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance"

xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/guf/1.0/core ../guf.xsd">

<itemIdentifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>GCL2000\_feedack\_item\_1</gco:CharacterString>

</mcc:code>

</mcc:MD\_Identifier>

</itemIdentifier>

<abstract>

<gco:CharacterString>Comparson with other land cover products is difficults because legends are not compatible</gco:CharacterString>

</abstract>

<contactRole>

<GUF\_UserRoleCode codeListValue="researchEndUser" codeList="">researchEndUser</GUF\_UserRoleCode>

</contactRole>

<dateInfo>

<cit:CI\_Date>

<cit:date><gco:DateTime>2006-03-01T00:00:00Z</gco:DateTime></cit:date>

<cit:dateType>

<cit:CI\_DateTypeCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_DateTypeCode" codeListValue="creation"/>

</cit:dateType>

</cit:CI\_Date>

</dateInfo>

<citation>

<cit:CI\_Citation>

<cit:title>

<gco:CharacterString>Towards the global monitoring of biodiversity change</gco:CharacterString>

</cit:title>

<cit:date>

<cit:CI\_Date>

<cit:date>

<gco:DateTime>2006-03-01T00:00:00Z</gco:DateTime>

</cit:date>

<cit:dateType>

<cit:CI\_DateTypeCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_DateTypeCode" codeListValue="creation"/>

</cit:dateType>

</cit:CI\_Date>

</cit:date>

<cit:series>

<cit:CI\_Series>

<cit:name>

<gco:CharacterString>TRENDS in Ecology and Evolution</gco:CharacterString>

</cit:name>

</cit:CI\_Series>

</cit:series>

<cit:otherCitationDetails>

<gco:CharacterString>Vol.21 No.3</gco:CharacterString>

</cit:otherCitationDetails>

</cit:CI\_Citation>

</citation>

<contact>

<GUF\_UserInformation>

<userDetails>

<cit:CI\_Responsibility>

<cit:role>

<cit:CI\_RoleCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_RoleCode" codeListValue="user"/>

</cit:role>

<cit:party>

<cit:CI\_Individual>

<cit:name>

<gco:CharacterString>Henrique M. Pereira</gco:CharacterString>

</cit:name>

</cit:CI\_Individual>

</cit:party>

</cit:CI\_Responsibility>

</userDetails>

<expertiseLevel>

<GUF\_RatingCode codeListValue="5" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_RatingCode"></GUF\_RatingCode>

</expertiseLevel>

</GUF\_UserInformation>

</contact>

<userComment>

<GUF\_UserComment>

<comment>

<gco:CharacterString>Surprisingly, there are no directly comparable sets of global land-cover data for two different

dates. For instance, the Global Land Cover for the year 2000 (GLC 2000) based on SPOT VEGETATION (http://www-gvm.jrc.it/glc2000) is not directly comparable

with the International Geosphere–Biosphere Programme (IGBP) Land Cover (1992–1993, http://edcdaac.usgs.gov/glcc/globdoc2\_0.asp) based on the National Oceanic

and Atmospheric Administration Advanced Very High Resolution Radiometer (NOAA-AVHRR). The difﬁculties arise from the use of different sensors, different land-cover

classiﬁcation systems (including different deﬁnitions of forest) and different classiﬁcation methods. </gco:CharacterString>

</comment>

</GUF\_UserComment>

</userComment>

<target>

<GUF\_FeedbackTarget>

<resourceRef xlink:href="http://www-gvm.jrc.it/glc2000">

<cit:CI\_Citation>

<cit:title></cit:title>

<cit:identifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>GLC2000</gco:CharacterString>

</mcc:code>

<mcc:codeSpace>

<gco:CharacterString>jrc.ec.europa.eu</gco:CharacterString>

</mcc:codeSpace>

</mcc:MD\_Identifier>

</cit:identifier>

</cit:CI\_Citation>

</resourceRef>

<scope>

<mcc:MD\_Scope>

<mcc:level>

<mcc:MD\_ScopeCode codeListValue="dataset" codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode"/>

</mcc:level>

</mcc:MD\_Scope>

</scope>

<role>

<GUF\_TargetRoleCode codeListValue="primary" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_TargetRoleCode"></GUF\_TargetRoleCode>

</role>

</GUF\_FeedbackTarget>

</target>

<target>

<GUF\_FeedbackTarget>

<resourceRef xlink:href="http://edcdaac.usgs.gov/glcc/globdoc2\_0.asp"/>

<scope>

<mcc:MD\_Scope>

<mcc:level>

<mcc:MD\_ScopeCode codeListValue="dataset" codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode"/>

</mcc:level>

</mcc:MD\_Scope>

</scope>

<role>

<GUF\_TargetRoleCode codeListValue="primary" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_TargetRoleCode"></GUF\_TargetRoleCode>

</role>

</GUF\_FeedbackTarget>

</target>

</GUF\_FeedbackItem>

# Geospatial User feedback model: Extensions

This section describes two requirements classes that are considered extensions of the XML encoding core: the User Feedback Summary and the User Feedback Collection.

## Requirements Class User Feedback Summary Extension

This requirements class defines the XML encoding classes that allow for encoding summary statistics of feedback items that share the same target.

1. /req/feedback-summary/ufs-schema:  
   An XML Encoding of a geospatial user feedback summary shall use UFS\_FeedbackSummary and shall validate using the geospatial user feedback summary schema ufs.xsd  
   Dependencies: /req/feedback-item  
   http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-summary

The ufs.xsd schema has been derived automatically from the OGC 15-097 UML model. No tables describing the naming of the elements and subelements are reproduced here as they are specified in the conceptual model.

The following code shows a xml encoding example for UFS\_FeedbackSummary.

<UFS\_FeedbackSummary

xmlns:mcc="http://standards.iso.org/iso/19115/-3/mcc/1.0"

xmlns:mri="http://standards.iso.org/iso/19115/-3/mri/1.0"

xmlns:cit="http://standards.iso.org/iso/19115/-3/cit/1.0"

xmlns:gco="http://standards.iso.org/iso/19115/-3/gco/1.0"

xmlns:guf="http://www.opengis.net/guf/1.0/core"

xmlns="http://www.opengis.net/guf/1.0/summary"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/guf/1.0/summary ../ufs.xsd">

<target>

<cit:CI\_Citation>

<cit:title></cit:title>

<cit:identifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>GLC2000</gco:CharacterString>

</mcc:code>

<mcc:codeSpace>

<gco:CharacterString>jrc.ec.europa.eu</gco:CharacterString>

</mcc:codeSpace>

</mcc:MD\_Identifier>

</cit:identifier>

</cit:CI\_Citation>

</target>

<numberOfFeedbackItems><gco:Integer>4</gco:Integer></numberOfFeedbackItems>

<minimumPossibleRating><gco:Real>1.0</gco:Real></minimumPossibleRating>

<maximumPossibleRating><gco:Real>5.0</gco:Real></maximumPossibleRating>

<averageRating><gco:Real>5.0</gco:Real></averageRating>

<numberOfRatings><gco:Integer>0</gco:Integer></numberOfRatings>

<numberOfUserComments><gco:Integer>3</gco:Integer></numberOfUserComments>

<numberOfUsageReports><gco:Integer>2</gco:Integer></numberOfUsageReports>

<numberOfCitations><gco:Integer>4</gco:Integer></numberOfCitations>

<numberOfAdditionalQualities><gco:Integer>3</gco:Integer></numberOfAdditionalQualities>

<numberOfAdditionalLineages><gco:Integer>0</gco:Integer></numberOfAdditionalLineages>

<numberOfSignificantEvents><gco:Integer>0</gco:Integer></numberOfSignificantEvents>

</UFS\_FeedbackSummary>

## Requirements Class User Feedback Collection Extension

This requirements class defines the XML encoding classes that allow for grouping of feedback items into a feedback response and feedback collection with summary statistics. A feedback collection is a collection of a feedback items that share a common target and share the same rating code list.

1. /req/feedback-collection/ufc-schema:  
   An XML Encoding of a geospatial user feedback collection shall use UFC\_FeedbackCollection and shall validate using the geospatial user feedback collection schema ufc.xsd  
   Dependencies: /req/feedback-collection  
   http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-collection

The ufc.xsd schema has been derived automatically from the OGC 15-097 UML model. No tables describing the naming of the elements and subelements are reproduced here as they are specified in the conceptual model.

The following code shows a xml encoding example for UFC\_FeedbackCollection.

<?xml version="1.0" encoding="UTF-8"?>

<UFC\_FeedbackCollection

xmlns:mcc="http://standards.iso.org/iso/19115/-3/mcc/1.0"

xmlns:mdq="http://standards.iso.org/iso/19157/-2/mdq/1.0"

xmlns:mri="http://standards.iso.org/iso/19115/-3/mri/1.0"

xmlns:cit="http://standards.iso.org/iso/19115/-3/cit/1.0"

xmlns:gco="http://standards.iso.org/iso/19115/-3/gco/1.0"

xmlns:qcm="http://www.opengis.net/guf/1.0/common"

xmlns:guf="http://www.opengis.net/guf/1.0/core"

xmlns="http://www.opengis.net/guf/1.0/collection"

xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xlink="http://www.w3.org/1999/xlink"

xsi:schemaLocation="http://www.opengis.net/guf/1.0/collection ../ufc.xsd">

<item>

<guf:GUF\_FeedbackItem>

<guf:itemIdentifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>GCL2000\_feedack\_item\_2</gco:CharacterString>

</mcc:code>

</mcc:MD\_Identifier>

</guf:itemIdentifier>

<guf:abstract>

<gco:CharacterString>Comparing several global land cover products, i.e. the Global Land Cover Characterization Database (GLCC), Global Land Cover 2000 (GLC2000), and the MODIS land cover product, reveil individual strengths and weaknesses of mapping approaches.</gco:CharacterString>

</guf:abstract>

<guf:contactRole>

<guf:GUF\_UserRoleCode codeListValue="researchEndUser" codeList="">researchEndUser</guf:GUF\_UserRoleCode>

</guf:contactRole>

<guf:dateInfo>

<cit:CI\_Date>

<cit:date>

<gco:DateTime>2006-01-01T00:00:00Z</gco:DateTime>

</cit:date>

<cit:dateType>

<cit:CI\_DateTypeCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_DateTypeCode" codeListValue="creation"/>

</cit:dateType>

</cit:CI\_Date>

</guf:dateInfo>

<guf:citation>

<cit:CI\_Citation>

<cit:title>

<gco:CharacterString>Exploiting synergies of global land cover products for carbon cycle modeling</gco:CharacterString>

</cit:title>

<cit:date>

<cit:CI\_Date>

<cit:date>

<gco:DateTime>2006-01-01T00:00:00Z</gco:DateTime>

</cit:date>

<cit:dateType>

<cit:CI\_DateTypeCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_DateTypeCode" codeListValue="creation"/>

</cit:dateType>

</cit:CI\_Date>

</cit:date>

<cit:series>

<cit:CI\_Series>

<cit:name>

<gco:CharacterString>Remote Sensing of Environment</gco:CharacterString>

</cit:name>

</cit:CI\_Series>

</cit:series>

<cit:otherCitationDetails>

<gco:CharacterString>101 (2006) 534–553</gco:CharacterString>

</cit:otherCitationDetails>

</cit:CI\_Citation>

</guf:citation>

<guf:additionalQuality>

<mdq:DQ\_DataQuality><mdq:scope><mcc:MD\_Scope>

<mcc:level><mcc:MD\_ScopeCode codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode" codeListValue="dataset"/></mcc:level>

</mcc:MD\_Scope></mdq:scope>

<mdq:report><mdq:DQ\_DomainConsistency>

<mdq:result>

<mdq:DQ\_DescriptiveResult>

<mdq:statement><gco:CharacterString>14% of the area of the GLCC, GLC2000, and MODIS land cover maps, reclassified to the SIMPLE legend disagree in the all three land cover maps. Areas where all maps disagree or only two maps agree seem to be associated with mainly transitional ecozones with mixtures of the three main components trees, shrubs and grasses such as tropical savannas including the Sahel, Mediterranean Europe, and tundra.</gco:CharacterString></mdq:statement>

</mdq:DQ\_DescriptiveResult>

</mdq:result>

</mdq:DQ\_DomainConsistency></mdq:report>

</mdq:DQ\_DataQuality>

</guf:additionalQuality>

<guf:usage>

<guf:GUF\_UsageReport>

<guf:usageDescription>

<mri:MD\_Usage>

<mri:specificUsage><gco:CharacterString>GLCC, GLC2000 and MODIS land cover products comparison</gco:CharacterString></mri:specificUsage>

</mri:MD\_Usage>

</guf:usageDescription>

<guf:discoveredIssue>

<qcm:QCM\_DiscoveredIssue>

<qcm:knownProblem>

<gco:CharacterString>None of legends of all three global land cover products are easily translated into the land cover classes of vegetation models without introducing uncertainty due to poor definition of mixed

classes or a lack of information about leaf type and phenology.</gco:CharacterString>

</qcm:knownProblem>

</qcm:QCM\_DiscoveredIssue>

</guf:discoveredIssue>

</guf:GUF\_UsageReport>

</guf:usage>

<guf:contact>

<guf:GUF\_UserInformation>

<guf:userDetails>

<cit:CI\_Responsibility>

<cit:role>

<cit:CI\_RoleCode codeList="http://wis.wmo.int/2008/catalogues/draft\_version\_1-1/WMO\_Codelists\_ver1\_1.xml#CI\_RoleCode" codeListValue="user"/>

</cit:role>

<cit:party>

<cit:CI\_Individual>

<cit:name>

<gco:CharacterString>Martin Jung</gco:CharacterString>

</cit:name>

</cit:CI\_Individual>

</cit:party>

</cit:CI\_Responsibility>

</guf:userDetails>

<guf:expertiseLevel>

<guf:GUF\_RatingCode codeListValue="5" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_RatingCode"></guf:GUF\_RatingCode>

</guf:expertiseLevel>

</guf:GUF\_UserInformation>

</guf:contact>

<guf:userComment>

<guf:GUF\_UserComment>

<guf:comment>

<gco:CharacterString> GLCC is based on poorly or uncorrected raw data, using only monthly NDVI composites that also have

some geometric problems. The VEGA data set of GLC2000 with daily composites of calibrated spectral bands and NDVI offers significantly improved data and more flexibility for

classification. A further advantage of the VEGA2000 is the effective geometric correction procedures (Bartholomé &amp; Belward, 2005). The input data sets of the MODIS product

supersede GLCC and GLC2000 in terms of the spectral properties of the MODIS instrument, specifically designed for land surface mapping. Also, the MODIS data are based on

higher spatial resolution of the raw data (250m/500m) and comprehensive strategies of data correction and calibration. Regarding the applied classification methods, MLCCA (MODIS land cover classification algorithm)

clearly seems the most sophisticated algorithm. In contrast to GLCC and GLC2000, it is purely objective, reproducible and operational for the whole globe, thus seems most suitable for change detection. GLCC offers the most flexibility for users in terms

of available reclassifications including the Olsen classification with 94 classes. MODIS is also available in different legends, which is not the case for GLC2000. LCCS of GLC2000 is the

most advanced and flexible classification system with a clear rationale and standardized definition of the classes. Although GLC2000 benefits strongly

from the use of LCCS and its regional bottom-up approach, its global map lacks some internal consistency associated with the individual mapping initiatives by different project participants.</gco:CharacterString>

</guf:comment>

</guf:GUF\_UserComment>

</guf:userComment>

<guf:target>

<guf:GUF\_FeedbackTarget>

<guf:resourceRef xlink:href="http://www-gvm.jrc.it/glc2000">

<cit:CI\_Citation>

<cit:title></cit:title>

<cit:identifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>GLC2000</gco:CharacterString>

</mcc:code>

<mcc:codeSpace>

<gco:CharacterString>jrc.ec.europa.eu</gco:CharacterString>

</mcc:codeSpace>

</mcc:MD\_Identifier>

</cit:identifier>

</cit:CI\_Citation>

</guf:resourceRef>

<guf:scope>

<mcc:MD\_Scope>

<mcc:level>

<mcc:MD\_ScopeCode codeListValue="dataset" codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode"/>

</mcc:level>

</mcc:MD\_Scope>

</guf:scope>

<guf:role>

<guf:GUF\_TargetRoleCode codeListValue="primary" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_TargetRoleCode"></guf:GUF\_TargetRoleCode>

</guf:role>

</guf:GUF\_FeedbackTarget>

</guf:target>

<guf:target>

<guf:GUF\_FeedbackTarget>

<guf:resourceRef xlink:href="http://edcdaac.usgs.gov/glcc/globdoc2\_0.asp">

<cit:CI\_Citation>

<cit:title></cit:title>

<cit:identifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>Global Land Cover Characterization DataBase (GLCC)</gco:CharacterString>

</mcc:code>

</mcc:MD\_Identifier>

</cit:identifier>

</cit:CI\_Citation>

</guf:resourceRef>

<guf:scope>

<mcc:MD\_Scope>

<mcc:level>

<mcc:MD\_ScopeCode codeListValue="dataset" codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode"/>

</mcc:level>

</mcc:MD\_Scope>

</guf:scope>

<guf:role>

<guf:GUF\_TargetRoleCode codeListValue="primary" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_TargetRoleCode"></guf:GUF\_TargetRoleCode>

</guf:role>

</guf:GUF\_FeedbackTarget>

</guf:target>

<guf:target>

<guf:GUF\_FeedbackTarget>

<guf:resourceRef>

<cit:CI\_Citation>

<cit:title></cit:title>

<cit:identifier>

<mcc:MD\_Identifier>

<mcc:code>

<gco:CharacterString>The MODIS land cover product</gco:CharacterString>

</mcc:code>

</mcc:MD\_Identifier>

</cit:identifier>

</cit:CI\_Citation>

</guf:resourceRef>

<guf:scope>

<mcc:MD\_Scope>

<mcc:level>

<mcc:MD\_ScopeCode codeListValue="dataset" codeList="http://standards.iso.org/iso/19115/resources/Codelist/cat/codeLists.xml#MD\_ScopeCode"/>

</mcc:level>

</mcc:MD\_Scope>

</guf:scope>

<guf:role>

<guf:GUF\_TargetRoleCode codeListValue="primary" codeList="http://www.opengis.net/guf/1.0/resources/codeList.xml#GUF\_TargetRoleCode"></guf:GUF\_TargetRoleCode>

</guf:role>

</guf:GUF\_FeedbackTarget>

</guf:target>

</guf:GUF\_FeedbackItem>

</item>

<pagination>

<UFC\_ResponsePagination>

<numberOfFeedbackItems><gco:Integer>1</gco:Integer></numberOfFeedbackItems>

<count><gco:Integer>1</gco:Integer></count>

</UFC\_ResponsePagination>

</pagination>

</UFC\_FeedbackCollection>

Annex A: Conformance Class Abstract Test Suite (Normative)

A GUF XML implementation of this standard must satisfy the following system characteristics to be conformant with this specification.

Conformance class: Quality Common

The OGC URI identifier of this conformance class is:

http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/quality-common

Tests identifiers below are relative to http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0

* + 1. MIME type

|  |  |
| --- | --- |
| **Test id:** | **conf/quality-common/mime-type** |
| **Test Purpose:** | **Req 1** /req/quality-common/mime-type: An XML encoding of a geospatial user feedback shall adopt the XML MIME type of application/xml |
| **Test method:** | Validate the MIME type  Test passes if the encoded instances have the associated MIME type application/xml. |

* + 1. File extension

|  |  |
| --- | --- |
| **Test id:** | **/conf/quality-common/file-extension** |
| **Test Purpose:** | **Req 2** /req/quality-common/file-extension: An XML encoding of a geospatial user feedback shall use the file extension ‘.xml’ |
| **Test method:** | Validate the file extension  Test passes if a file system is used and the encoded instances are files with ‘.xml’ file extension |

* + 1. ISO XML rules

|  |  |
| --- | --- |
| **Test id:** | **/conf/quality-common/xmlrules** |
| **Test Purpose:** | **Req 3** /req/quality-common/xmlrules: An XML encoding of a geospatial user feedback shall comply with the encoding rules specified in ISO-19139. Dependencies: ISO 19139 |
| **Test method:** | Validate the encoding rules followed  Test passes if the encoded instances follow ISO-19139 conformance classes. |

* + 1. ISO XML schema

|  |  |
| --- | --- |
| **Test id:** | **/conf/quality-common/iso-schema** |
| **Test Purpose:** | **Req 4** /req/quality-common/iso-schema: An XML encoding of a geospatial user feedback shall validate using the schemas ISO19115-3 and ISO19157-2 provided at: http://standards.iso.org/iso/19115/-3 and http://standards.iso.org/iso/19157/-2 respectively Dependencies: ISO 19115-3 and ISO 19157-2 |
| **Test method:** | Validate the XML against the right XML schema  Test passes if encoded instances validates under the ISO XML schemas for ISO19115-1 and ISO19157-1 that are provided by ISO19115-3 and ISO19157-2 respectively. |

* + 1. Quality common XML schema

|  |  |
| --- | --- |
| **Test id:** | **/conf/** **quality-common/qcm-schema** |
| **Test Purpose:** | **Req 5** /req/quality-common/qcm-schema: An XML encoding of a geospatial user feedback using QCM\_Publication or QCM\_DiscoveredIssue shall validate using the quality common schema qcm.xsd Dependencies: http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/quality-common |
| **Test method:** | Validate the XML against the right XML schema  Test passes if XML elements of the data type QCM\_Publication and QCM\_DiscoveredIssue conform to the http://www.opengis.net/spec/geospatial-user-feedback/1.0/conf/quality-common and validate against the quality common schema with the XML namespace http://www.opengis.net/guf/1.0/common and encoded in the qcm.xsd |

Conformance class: User Feedback-item

The OGC URI identifier of this conformance class is:

http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/feedback-item

Tests identifiers below are relative to http://www.opengis.net/spec/geospatial-user-feedback/1.0

* + 1. Feedback item XML schema

|  |  |
| --- | --- |
| **Test id:** | **/conf/feedback-item/item** |
| **Test Purpose:** | **Req 6** /req/feedback-item/guf-schema: An XML encoding of a geospatial user feedback item shall use GUF\_FeedbackItem and shall validate using the geospatial user feedback item schema guf.xsd Dependencies: /req/quality-common  http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-item |
| **Test method:** | Validate the XML against the right XML schema  Test passes if XML elements of the data type GUF\_FeedbackItem conform to the http://www.opengis.net/spec/geospatial-user-feedback/1.0/conf/feedback-item and validate against the quality common schema with the XML namespace http://www.opengis.net/guf/1.0/core and encoded in the guf.xsd |

Conformance class: Feedback-summary

The OGC URI identifier of this conformance class is:

http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/feedback-summary

Tests identifiers below are relative to http://www.opengis.net/spec/geospatial-user-feedback/1.0

* + 1. Feedback summary XML schema

|  |  |
| --- | --- |
| **Test id:** | **/conf/feedback-summary/summary-model** |
| **Test Purpose:** | **Req 7** /req/feedback-summary/ufs-schema: An XML Encoding of a geospatial user feedback summary shall use UFS\_FeedbackSummary and shall validate using the geospatial user feedback summary schema ufs.xsd Dependencies: /req/feedback-item http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-summary |
| **Test method:** | Validate the XML against the right XML schema  Test passes if XML elements of the data type UFS\_FeedbackSummary conform to the http://www.opengis.net/spec/geospatial-user-feedback/1.0/conf/feedback-summary and validate against the quality common schema with the XML namespace http://www.opengis.net/guf/1.0/summary and encoded in the ufs.xsd. |

Conformance class: Feedback-collection

The OGC URI identifier of this conformance class is:

http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0/conf/feedback-collection

Tests identifiers below are relative to http://www.opengis.net/spec/geospatial-user-feedback-xml/1.0

* + 1. Feedback collection XML schema

|  |  |
| --- | --- |
| **Test id:** | **/conf/feedback-collection/response** |
| **Test Purpose:** | **Req 8** /req/feedback-collection/ufc-schema: An XML Encoding of a geospatial user feedback collection shall use UFC\_FeedbackCollection and shall validate using the geospatial user feedback collection schema ufc.xsd Dependencies: /req/feedback-collection http://www.opengis.net/spec/geospatial-user-feedback/1.0/req/feedback-collection |
| **Test method:** | Validate the XML against the right XML schema  Test passes if XML elements of the data type UFC\_FeedbackCollection conform to the http://www.opengis.net/spec/geospatial-user-feedback/1.0/conf/feedback-collection and validate against the quality common schema with the XML namespace http://www.opengis.net/guf/1.0/collection and encoded in the ufc.xsd |

Annex B: XML Schema Documents

In addition to this document, this standard includes several XML Schema Documents. These XML Schema Documents are available at http://schemas.opengis.net/guf/1.0.

These XML Schema Documents and examples combine the XML schema fragments listed in various subclauses of this document, eliminating duplications. These XML Schema Documents match the GUF UML packages described in the OGC 15-097 Geospatial User Feedback Conceptual Model and were derived from them using ShapeChange application, and are named:

qcm.xsd

guf.xsd

ufs.xsd

ufc.xsd

These XML Schema Documents use and build on the ISO19115-3 and ISO19157-2 XML Schema Documents specified by ISO and that are available at http://standards.iso.org/iso, named:

19115/-3/mcc/1.0/mcc.xsd

19157/-2/mdq/1.0/mdq.xsd

19115/-3/gex/1.0/gex.xsd

19115/-3/mri/1.0/mri.xsd

19115/-3/cit/1.0/cit.xsd

19115/-3/gco/1.0/gco.xsd

19115/-3/mrl/1.0/mrl.xsd

19115/-3/lan/1.0/lan.xsd

19115/-3/mdb/1.0/mdb.xsd

All these XML Schema Documents contain documentation of the meaning of each element and attribute, and this documentation shall be considered normative as specified in Subclause 11.6.3 of [OGC 06-121r3].

Annex C: Revision history

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Date | Release | Author | Paragraph modified | Description |
| 2016-10-24 | 1.0 | Scott Simmons | Throughout document | Preparation for final publication |
|  |  |  |  |  |
|  |  |  |  |  |

Bibliography

OGC: OGC 08-131r3 The Specification Model — A Standard for Modular specifications (2009)

OGC: OGC 12-093 OWS-9: UML-to-GML-Application-Schema (UGAS) Conversion Engineering Report. Clemens Portele (ed.) (2013)

ShapeChange: Processing application schemas for geographic information. Website: http://shapechange.net/

1. http://schemas.geoviqua.org [↑](#footnote-ref-1)
2. [www.opengeospatial.org/cite](http://www.opengeospatial.org/cite) [↑](#footnote-ref-2)